(kicad_symbol_lib
  (version 20251024)
  (generator "Protoflow")
    (symbol "B2B-PH-K-S" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 -2.54 0))
      (property "Value" "B2B-PH-K-S" (id 1) (at 0 2.54 0))
      (property "Footprint" "ProtoFlow.pretty:JST_B2B-PH-K-S_1x02_P2.00mm_Vertical" (id 2) (at 0 0 0))
      (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf" (id 3) (at 0 0 0))
      (property "Description" "PH-series 2-contact top-entry through-hole shrouded header, 2.0 mm pitch, 2 A, 100 V" (id 4) (at 0 0 0))
      (property "ki_keywords" "JST PH connector header shrouded vertical through-hole wire-to-board" (id 5) (at 0 0 0))
      (property "Manufacturer" "J.S.T. Mfg. Co., Ltd." (id 6) (at 0 0 0))
      (property "MPN" "B2B-PH-K-S" (id 7) (at 0 0 0))
      (property "Package" "JST_B2B-PH-K-S_1x02_P2.00mm_Vertical" (id 8) (at 0 0 0))
      (property "Applicable PCB Thickness" "0.8 mm to 1.6 mm" (id 9) (at 0 0 0))
      (property "Current Rating" "2 A AC/DC with AWG 24 wire" (id 10) (at 0 0 0))
      (property "Initial Contact Resistance" "10 mΩ maximum" (id 11) (at 0 0 0))
      (property "Insulation Resistance" "1000 MΩ minimum" (id 12) (at 0 0 0))
      (property "Operating Temperature" "-40 °C to 105 °C including current-induced temperature rise" (id 13) (at 0 0 0))
      (property "Pitch" "2.0 mm" (id 14) (at 0 0 0))
      (property "Voltage Rating" "100 V AC/DC" (id 15) (at 0 0 0))
      (property "Withstanding Voltage" "800 V AC for 1 minute" (id 16) (at 0 0 0))
      (symbol "B2B-PH-K-S_1_1"
        (pin passive line (at -7.62 1.27 0) (length 3.81) (name "1") (number "1"))
        (pin passive line (at -7.62 -1.27 0) (length 3.81) (name "2") (number "2"))
      )
    )
)
