(footprint "JST_B2B-PH-K-S_1x02_P2.00mm_Vertical"
  (version 20221018)
  (generator "Protoflow")
  (layer "F.Cu")
  (fp_text reference "REF**" (at 0 -4.05) (layer "F.SilkS"))
  (fp_text value "B2B-PH-K-S" (at 0 2.95) (layer "F.Fab"))
  (pad "1" thru_hole circle (at 1 0) (size 1.3 1.3) (drill 0.7) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole circle (at -1 0) (size 1.3 1.3) (drill 0.7) (layers "*.Cu" "*.Mask"))
)
