(kicad_symbol_lib
  (version 20251024)
  (generator "Protoflow")
    (symbol "TPS62160DSG" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 -6.35 0))
      (property "Value" "TPS62160DSG" (id 1) (at 0 6.35 0))
      (property "Footprint" "ProtoFlow.pretty:WSON-8_DSG0008A_2x2mm_P0.5mm_EP_NoOptionalVias" (id 2) (at 0 0 0))
      (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62160.pdf" (id 3) (at 0 0 0))
      (property "Description" "Synchronous step-down converter, 3 V to 17 V input, adjustable 0.9 V to 6 V output, 1 A, WSON-8 with exposed pad" (id 4) (at 0 0 0))
      (property "ki_keywords" "buck synchronous adjustable regulator DCS-Control power-good WSON" (id 5) (at 0 0 0))
      (property "Manufacturer" "Texas Instruments" (id 6) (at 0 0 0))
      (property "MPN" "TPS62160DSG" (id 7) (at 0 0 0))
      (property "Package" "WSON-8_DSG0008A_2x2mm_P0.5mm_EP_NoOptionalVias" (id 8) (at 0 0 0))
      (property "Feedback Reference Voltage" "0.8 V" (id 9) (at 0 0 0))
      (property "Operating Junction Temperature" "-40 °C to 125 °C" (id 10) (at 0 0 0))
      (property "Output Current" "1 A" (id 11) (at 0 0 0))
      (property "Output Voltage" "0.9 V to 6 V" (id 12) (at 0 0 0))
      (property "Quiescent Current" "17 µA typical" (id 13) (at 0 0 0))
      (property "Supply Voltage" "3 V to 17 V" (id 14) (at 0 0 0))
      (property "Switching Frequency" "2.25 MHz typical" (id 15) (at 0 0 0))
      (symbol "TPS62160DSG_1_1"
        (pin input line (at -12.7 2.54 0) (length 3.81) (name "EN") (number "3"))
        (pin input line (at -12.7 0 0) (length 3.81) (name "VOS") (number "6"))
        (pin input line (at -12.7 -2.54 0) (length 3.81) (name "FB") (number "5"))
        (pin output line (at 12.7 1.27 180) (length 3.81) (name "SW") (number "7"))
        (pin open_collector line (at 12.7 -1.27 180) (length 3.81) (name "PG") (number "8"))
        (pin power_in line (at 0 8.89 270) (length 3.81) (name "VIN") (number "2"))
        (pin power_in line (at -2.54 -8.89 90) (length 3.81) (name "PGND") (number "1"))
        (pin power_in line (at 0 -8.89 90) (length 3.81) (name "AGND") (number "4"))
        (pin power_in line (at 2.54 -8.89 90) (length 3.81) (name "EP") (number "9"))
      )
    )
)
