(footprint "WSON-8_DSG0008A_2x2mm_P0.5mm_EP_NoOptionalVias"
  (version 20221018)
  (generator "Protoflow")
  (layer "F.Cu")
  (fp_text reference "REF**" (at 0 -2.25) (layer "F.SilkS"))
  (fp_text value "TPS62160DSG" (at 0 2.25) (layer "F.Fab"))
  (pad "1" smd roundrect (at -0.95 -0.75) (size 0.5 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "2" smd roundrect (at -0.95 -0.25) (size 0.5 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "3" smd roundrect (at -0.95 0.25) (size 0.5 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "4" smd roundrect (at -0.95 0.75) (size 0.5 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "5" smd roundrect (at 0.95 0.75) (size 0.5 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "6" smd roundrect (at 0.95 0.25) (size 0.5 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "7" smd roundrect (at 0.95 -0.25) (size 0.5 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "8" smd roundrect (at 0.95 -0.75) (size 0.5 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2))
  (pad "9" smd roundrect (at 0 0) (size 0.9 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.055556))
)
