(kicad_symbol_lib
  (version 20251024)
  (generator "Protoflow")
    (symbol "AMS1117-3.3" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 -2.54 0))
      (property "Value" "AMS1117-3.3" (id 1) (at 0 2.54 0))
      (property "Footprint" "ProtoFlow.pretty:SOT-223-3_TabPin2" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf" (id 3) (at 0 0 0))
      (property "Description" "Fixed 3.3 V low-dropout linear regulator, 1 A, SOT-223" (id 4) (at 0 0 0))
      (property "ki_keywords" "LDO linear regulator fixed positive 3.3V SOT223" (id 5) (at 0 0 0))
      (property "Manufacturer" "Advanced Monolithic Systems, Inc." (id 6) (at 0 0 0))
      (property "MPN" "AMS1117-3.3" (id 7) (at 0 0 0))
      (property "Package" "SOT-223-3_TabPin2" (id 8) (at 0 0 0))
      (property "Dropout Voltage" "1.3 V maximum at 1 A" (id 9) (at 0 0 0))
      (property "Input Voltage Absolute Maximum" "15 V" (id 10) (at 0 0 0))
      (property "Operating Junction Temperature" "-40 °C to 125 °C" (id 11) (at 0 0 0))
      (property "Output Current" "1 A" (id 12) (at 0 0 0))
      (property "Output Voltage" "3.3 V" (id 13) (at 0 0 0))
      (property "Quiescent Current" "5 mA typical, 11 mA maximum" (id 14) (at 0 0 0))
      (symbol "AMS1117-3.3_1_1"
        (pin power_in line (at -11.43 0 0) (length 3.81) (name "VIN") (number "3"))
        (pin power_out line (at 11.43 0 180) (length 3.81) (name "VOUT") (number "2"))
        (pin power_in line (at 0 -7.62 90) (length 3.81) (name "GND") (number "1"))
      )
    )
)
